SMARTSOURCE MANAGER


SMARTSOURCE KERNEL:

The release notes contained in this folder apply to the Standard CAPI Installation.

The SmartSource Kernel differs from the Standard and Minimum CAPI Installation in the following ways:

- All filenames conform to the 8.3 file naming convention.
	- SmartSourceManager.exe is renamed as SSMng.exe
	- ZFPGA_DL2.rbf is renamed as ZFPGA_02.rbf. The device.ini references this new filename.

- Only Adaptive supported - not Professional or Value.

- CCITT threshold 8 supported: other thresholds 0-7 and 9-15 are not supported.

- MICR only, No OCR supported.

- No built-in endorser font. Endorser can use TrueType fonts only

- No Trace Dump Utility (However, ‘T’ and<ENTER> in Manager console window will dump unzipped trace files).

- No Exception Handler.

- No support for SmartSource Intelligence.

- No SmartStats utility - error logs will not be created.

- No Windows Control Utility (SmartSourceStart.exe or SmartSourceStartup.exe) - manager console window will be displayed, not hidden.

- No Trace Trigger utility.

- No Exception Viewer.

- No Error Database Conversion Utility.

- No ImageView utility.

- No Exerciser utility.

- No CAPI MICR/OCR Codeline TrueType font (This font is used by Exerciser/Exception Handler).

- No entries in the Start menu

- Qualified on 32 bit XP Professional Operating System only


----------------------------------
SOFTWARE INSTALLATION INSTRUCTIONS
----------------------------------

The Track PC must be running Microsoft Windows XP Professional Edition for the Adaptive Kernel.

1. You must have Administrator to run the installation. Before installing the software, stop all other applications 
and power off the SmartSource unit. 
To install the software, run setup.exe

2. The user account that will run this software must be assigned full control permissions to the folder
where the software was installed (eg, C:\SmartSource) and its subfolders, as well as the folder where images will be stored 
(for the image storage path, see the values of DriveLetter and StoragePathName in the registry, HKLM\Software\Unisys\SmartSource).

The USB connection must be USB 2.0.


Regarding Anti-Virus Software:

The Track PC is operating realtime applications that require unfettered access to each other and their associated PC's.
Their performance can be severely impacted by active agents of antivirus software programs. 
Periodic scans can be run (ie: once per day, or once per week) when the transport is not processing live work, 
but should never be left running while these systems are in use.


Regarding Screen Savers:

Screen Savers should not be run while the Transport PC is in use. 
